# KT1025AHow to modify the prompt sound to your own needs

# 1. Instructions for prompt sounds

1. At present, there are five prompt tones supported in the chip.

|  |  |  |
| --- | --- | --- |
| Music mode | Music.mp3 |  |
| Bluetooth mode | Bt.mp3 |  |
| Successful connection | Connect.mp3 |  |
| Connection disconnect | Disconnect.mp3 |  |
| Incoming call | Ring.mp3 |  |

2. If you need to change the prompt tone, please provide the above file. The file must be compressed.Must be named as above

The size of 3 and 5 files can not exceed 17KB, which is limited by the memory space inside the chip.

4. The volume of the prompt sound should be edited by software.You can put it in the TF card and play it. Is the sound appropriate?

5. In order to facilitate the use of customers, the specific effect can be audited by BT201 module.**Hint tones we use are monotones**

6. If you don&apos;t need prompt tone, you can turn it off by serial instructions. See the manual for details.

# Explanation of customized prompt sound

1. If you need to customize the prompt tone, this can only be us, because the prompt tone is written in the chip, the user can not modify it.

2. There are three requirements to modify the prompt sound:

(1) Provide us with prompt sound, we must pack and send to us in accordance with the above requirements, note the information, after we improve, new procedures will be upgraded to you.

(2) The user&apos;s product must be a product. If you make a sample casually, it is not necessary for us to modify it.After all, manpower is also a cost.

You&apos;ll see.

(3) If there are some special tips, it is necessary for us to charge for them, so you should consider them well.